# Lids

## Switches

### MX key switches

> [!NOTE]  
> the mx switch lids are too tall to be used as a lid for the bin containing the microcontroller. Either use a lid with a different sensor or a blank lid. 

#### 1x1 round mx switch

![round-mx-key](https://github.com/user-attachments/assets/0d917087-21ff-4c26-b0a9-f32d2f6f3d86)

Use with mx-switch-round-cap-23mm.

#### 1x1 square mx switch

![square-mx-switch](https://github.com/user-attachments/assets/1ea6a703-620f-4e8e-b87d-ada5feed8370)

Use with mx-switch-square-cap-33x33mm.

#### 1x1 2 mx switches

![two-mx-switches](https://github.com/user-attachments/assets/96080e49-99f1-488b-b090-8cc5584aa161)

Use with mx-switch-square-cap-15x33mm.

#### 1x1 4 mx switches

![four-mx-keys](https://github.com/user-attachments/assets/66227468-aff2-439b-9f2a-dfe1a6d98079)

Use with mx-switch-square-cap-15x15mm.

#### 2x1 8 mx switches

![eight-mx-switches](https://github.com/user-attachments/assets/3c29489d-aed7-4dfd-9d7b-b15f0b13cd93)

Use with mx-switch-square-cap-15x15mm.

### Self-locking 8x8mm switch

#### 1x1 round self-locking switch

![round-lock-switch](https://github.com/user-attachments/assets/2db9126a-7a15-454f-b495-049386368cd5)


Use with switch-lock-round-cap-23mm.

### Rotary encoder

#### 1x1 rotary encoder

![rotary-encoder](https://github.com/user-attachments/assets/71e3282d-cf01-481a-a143-e656c34fc811)

Use with rotary-encoder-cap-15mm.

#### 1x1 4 rotary encoders

![four-rotary-encoders](https://github.com/user-attachments/assets/a92af47c-9342-4e72-b5de-7dede6285f84)

Use with rotary-encoder-cap-15mm.

### Slider potentiometer

Use with slider-cap-18mm.

#### 2x1 75mm slider potentiometer

![slider](https://github.com/user-attachments/assets/e280cec2-2faa-49ae-88bf-b97bb8a23d37)

Use with slider-cap-18mm.
