---
title: Yamaha MusicCast
toc_min_heading_level: 2
toc_max_heading_level: 5
---

import Tabs from '@theme/Tabs';
import TabItem from '@theme/TabItem';
import CodeBlock from '@theme/CodeBlock';
import JsonConfig from '!!raw-loader!@site/../config/musiccast.json.example';

Monitor [MusicCast](https://usa.yamaha.com/products/contents/audio_visual/musiccast/index.html) device/receivers for music played on Network/USB/CD inputs.

:::tip[Scrobbling Threshold]

Musiccast may not correctly report track length. If this is the case you should reduce the "listened to" **duration** using [Scrobble Thresholds](/configuration/sources#scrobble-thresholds) so that multi-scrobbler scrobbles correctly.

:::

##### URL

If only a domain/IP:PORT is provided to multi-scrobbler it will automatically append the default Musiccast API path. If your Musiccast device is located behind a custom URL (or reverse proxy) you should explicitly provide the base path to use.

EX

    | `url`                                   | Transformed URL                                 |
    | --------------------------------------- | :---------------------------------------------- |
    | `http://192.168.0.101`                  | `http://192.168.0.101/YamahaExtendedControl/v1` |
    | `http://mydomain.com/reverseProxy/cast` | `http://mydomain.com/reverseProxy/cast`         |

## Configuration

<Config config="MusicCastSourceConfig" fileContent={JsonConfig} name="musiccast">
        | Environmental Variable | Required? | Default | Description              |
        | :--------------------- | :-------- | ------- | :----------------------- |
        | `MCAST_URL`            | Yes       |         | The Musiccast device URL |  
</Config>