# importAWGFile

Import numeric data from a text file as column vectors. Can be used to import data defining an arbitrary waveform from a file.

This function was auto-generated by MATLAB on 2013/11/06 17:37:04

## Contents

- Syntax
- Description
- Examples
- Input Arguments
- Output Arguments
- See Also

## Syntax

AWGARRAY = importAWGFile(FILENAME)

AWGARRAY = importAWGFile(FILENAME, STARTROW, ENDROW)

## Description

AWGARRAY = importAWGFile(FILENAME) Reads data from text file FILENAME for the default selection.

AWGARRAY = importAWGFile(FILENAME, STARTROW, ENDROW) Reads data from rows STARTROW through ENDROW of text file FILENAME.

## Examples

    awgArray = importAWGFile('2205A_AWG_Sine.csv');
    whos;

    awgArray = importAWGFile('2205A_AWG_Sine.csv', 1, 2048);
    whos;

      Name                      Size             Bytes  Class     Attributes

      B                         1x1                  8  double
      D                         1x1                  8  double
      F                         1x1                  8  double
      P                         1x1                  4  uint32
      Q                         1x25                50  char
      R                         1x1                  8  double
      T                         1x1                  8  double
      U                         1x2                  4  char
      W                         1x1                  8  double
      X                         1x1                  2  char
      Y                         1x11                22  char
      ans                       1x177              354  char
      awgArray               4096x1              32768  double
      flag                      1x1                  8  double
      maxValue                  1x1                  8  double
      n                         1x1                  8  double
      psTbxProject              1x1               1712  struct
      psTbx_doc_options         1x1                829  struct
      rootDir                   1x143              286  char
      voltageRange              1x1                  8  double

      Name                      Size             Bytes  Class     Attributes

      B                         1x1                  8  double
      D                         1x1                  8  double
      F                         1x1                  8  double
      P                         1x1                  4  uint32
      Q                         1x25                50  char
      R                         1x1                  8  double
      T                         1x1                  8  double
      U                         1x2                  4  char
      W                         1x1                  8  double
      X                         1x1                  2  char
      Y                         1x11                22  char
      ans                       1x177              354  char
      awgArray               2048x1              16384  double
      flag                      1x1                  8  double
      maxValue                  1x1                  8  double
      n                         1x1                  8  double
      psTbxProject              1x1               1712  struct
      psTbx_doc_options         1x1                829  struct
      rootDir                   1x143              286  char
      voltageRange              1x1                  8  double

## Input Arguments

- FILENAME - name of the file from which data is to be read (string)
- STARTROW - first row to read data from (scalar integer)
- ENDROW - last row to read data from (scalar integer)

## Output Arguments

- AWGARRAY - column vector of numeric data read from FILENAME

## See Also

`textscan`

Copyright: © 2015 Pico Technology Ltd. All rights reserved.