# Functions

## Contents

- Data Conversion Functions
- Other Functions

## Data Conversion Functions

- `adc2mv`: Converts raw Analog to Digital Converter count values to millivolts.
- `freq2delta`: Convert frequency to delta value for PicoScope Arbitrary Waveform Generators.
- `mv2adc`: Converts millivolt values to Analog to Digital Converter count values.
- `normalise`: Normalize a vector or matrix.

## Other Functions

- `getVerticalAxisLabel`: Obtain a label to use on a vertical axis of a plot
- `importAWGFile`: Import numeric data from a text file as column vectors.
- `questionDialog`: Dialog prompting a User to respond 'Yes' or 'No' to a question.
- `stopButton`: Displays a stop button.
- `timeunits`: Returns a string representation of the time unit index.

Copyright: © 2015-2019 Pico Technology Ltd. All rights reserved.