---
title: MPRIS
toc_min_heading_level: 2
toc_max_heading_level: 5
---

import Tabs from '@theme/Tabs';
import TabItem from '@theme/TabItem';
import CodeBlock from '@theme/CodeBlock';
import MPRISConfig from '!!raw-loader!@site/../config/mpris.json.example';

[MPRIS](https://specifications.freedesktop.org/mpris-spec/latest) is a standard interface for communicating with Music Players on **linux operating systems.**

If you run Linux and have a notification tray that shows what media you are listening to, you likely have access to MPRIS.

![Notification Tray](../mpris.jpg)

multi-scrobbler can listen to this interface and scrobble tracks played by **any media player** that communicates to the operating system with MPRIS.

##### Host Setup

MPRIS communication requires multi-scrobbler to have access to the host's dbus-daemon.

<Tabs groupId="dbus" queryString>
    <TabItem value="local" label="Local">
        If multi-scrobbler is running as a [**Local Installation**](../../installation/installation.mdx#nodejs), directly with node/npm, on the same host as MPRIS then no setup is required.

        Remote setup is also possible, see the **Remote Unix Socket** section in the Docker tab.
    </TabItem>
    <TabItem value="docker" label="Docker">
        If multi-scrobbler is running as a [**Docker Container**](../../installation/installation.mdx#docker) some modifications are required...

        ##### Local Unix Socket

        The most secure way is to **run a multi-scrobbler container on the same host as MPRIS.** In this scenario you can simply mount the **user session** dbus unix socket into the container. Make sure [`PUID` and `PGID` ENVs are configured](/installation?dockerSetting=linuxHost#recommended-settings) so the container has permissions to access the socket. Then, modify your compose stack with these additional values:

        ```yaml title="docker-compose.yaml"

            environment:
            - DBUS_SESSION_BUS_ADDRESS=unix:path=/run/user/UID/bus 

            volumes:
            - /run/user/UID/bus:/run/user/UID/bus:ro
        ```

        ##### Remote Unix Socket

        :::warning

        This method is **insecure.** You should not expose dbus over a network unless access to the port is restricted and the network is trusted.

        :::

        Use [`socat`](https://linux.die.net/man/1/socat) to bidirectionally relay communication from the host's dbus socket to a listening TCP port.

        To make dbus for user with uid `1000` available on port `6644`:

        ```shell
        socat TCP-LISTEN:6644,reuseaddr,fork UNIX-CONNECT:/run/user/1000/bus
        ```

        Then, add the following value to multi-scrobbler's ENVs:

        ```
        DBUS_SESSION_BUS_ADDRESS=tcp:host=yourHostIP,port=6644
        ```

    </TabItem>
</Tabs>

## Configuration

<Config config="MPRISSourceConfig" fileContent={MPRISConfig} name="mpris">
        | Environmental Variable | Required? | Default | Description                                                                      |
        |------------------------|-----------|---------|----------------------------------------------------------------------------------|
        | MPRIS_ENABLE           | No        |         | Use MPRIS as a Source (useful when you don't need any other options)             |
        | MPRIS_BLACKLIST        | No        |         | Comma-delimited list of player names not to scrobble from                        |
        | MPRIS_WHITELIST        | No        |         | Comma-delimited list of players names to ONLY scrobble from. Overrides blacklist |
</Config>